<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.4.1">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="67.31" y2="0" width="0" layer="20"/>
<wire x1="67.31" y1="0" x2="67.31" y2="38.1" width="0" layer="20"/>
<wire x1="67.31" y1="38.1" x2="0" y2="38.1" width="0" layer="20"/>
<wire x1="0" y1="38.1" x2="0" y2="0" width="0" layer="20"/>
</plain>
<libraries>
<library name="SparkFun-Capacitors">
<description>&lt;h3&gt;SparkFun Capacitors&lt;/h3&gt;
This library contains capacitors. 
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="0805">
<description>&lt;p&gt;&lt;b&gt;Generic 2012 (0805) package&lt;/b&gt;&lt;/p&gt;
&lt;p&gt;0.2mm courtyard excess rounded to nearest 0.05mm.&lt;/p&gt;</description>
</package>
</packages>
</library>
<library name="pinhead">
<description>&lt;b&gt;Pin Header Connectors&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="1X07">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
<package name="1X01">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
<package name="1X03">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="ISOW7842">
<packages>
<package name="DWE0016A">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="C1" library="SparkFun-Capacitors" package="0805" value="10uF">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="CAP-11330"/>
<attribute name="VALUE"/>
</element>
<element name="C2" library="SparkFun-Capacitors" package="0805" value="1.0uF">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="CAP-11625"/>
<attribute name="VALUE"/>
</element>
<element name="C3" library="SparkFun-Capacitors" package="0805" value="0.1uF">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="CAP-11625"/>
<attribute name="VALUE"/>
</element>
<element name="C4" library="SparkFun-Capacitors" package="0805" value="10uF">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="CAP-11330"/>
<attribute name="VALUE"/>
</element>
<element name="C5" library="SparkFun-Capacitors" package="0805" value="1.0uF">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="CAP-11625"/>
<attribute name="VALUE"/>
</element>
<element name="C6" library="SparkFun-Capacitors" package="0805" value="0.1uF">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="CAP-11625"/>
<attribute name="VALUE"/>
</element>
<element name="JP1" library="pinhead" package="1X07" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="JP10" library="pinhead" package="1X01" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="JP11" library="pinhead" package="1X01" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="JP12" library="pinhead" package="1X01" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="JP13" library="pinhead" package="1X01" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="JP14" library="pinhead" package="1X01" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="JP15" library="pinhead" package="1X01" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="JP16" library="pinhead" package="1X01" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="JP17" library="pinhead" package="1X01" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="JP18" library="pinhead" package="1X01" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="JP19" library="pinhead" package="1X01" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="JP2" library="pinhead" package="1X07" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="JP20" library="pinhead" package="1X01" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="JP3" library="pinhead" package="1X03" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="JP4" library="pinhead" package="1X03" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="JP5" library="pinhead" package="1X01" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="JP6" library="pinhead" package="1X01" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="JP7" library="pinhead" package="1X01" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="JP8" library="pinhead" package="1X01" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="JP9" library="pinhead" package="1X01" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U1" library="ISOW7842" package="DWE0016A" value="Value">
<attribute name="MANUFACTURER" value="Texas Instruments"/>
<attribute name="NAME"/>
<attribute name="PARTNUMBER" value="ISOW7842DWER"/>
<attribute name="REFDES" value="RefDes"/>
<attribute name="TYPE" value="TYPE"/>
</element>
</elements>
<signals>
<signal name="VCC1">
<contactref element="U1" pad="1"/>
<contactref element="JP5" pad="1"/>
<contactref element="JP1" pad="1"/>
<contactref element="C3" pad="1"/>
<contactref element="C2" pad="1"/>
<contactref element="C1" pad="1"/>
<contactref element="JP4" pad="1"/>
</signal>
<signal name="VCC2">
<contactref element="U1" pad="16"/>
<contactref element="JP20" pad="1"/>
<contactref element="JP2" pad="1"/>
<contactref element="C6" pad="1"/>
<contactref element="C5" pad="1"/>
<contactref element="C4" pad="1"/>
<contactref element="JP3" pad="1"/>
</signal>
<signal name="GND2">
<contactref element="U1" pad="9"/>
<contactref element="U1" pad="15"/>
<contactref element="JP19" pad="1"/>
<contactref element="JP2" pad="2"/>
<contactref element="C6" pad="2"/>
<contactref element="C5" pad="2"/>
<contactref element="C4" pad="2"/>
<contactref element="JP3" pad="3"/>
<contactref element="JP13" pad="1"/>
</signal>
<signal name="GND1">
<contactref element="U1" pad="2"/>
<contactref element="U1" pad="8"/>
<contactref element="JP6" pad="1"/>
<contactref element="JP1" pad="2"/>
<contactref element="JP12" pad="1"/>
<contactref element="JP4" pad="3"/>
<contactref element="C3" pad="2"/>
<contactref element="C2" pad="2"/>
<contactref element="C1" pad="2"/>
</signal>
<signal name="N$1">
<contactref element="U1" pad="3"/>
<contactref element="JP1" pad="3"/>
<contactref element="JP7" pad="1"/>
</signal>
<signal name="N$2">
<contactref element="U1" pad="5"/>
<contactref element="JP1" pad="5"/>
<contactref element="JP9" pad="1"/>
</signal>
<signal name="N$3">
<contactref element="U1" pad="4"/>
<contactref element="JP1" pad="4"/>
<contactref element="JP8" pad="1"/>
</signal>
<signal name="N$4">
<contactref element="U1" pad="6"/>
<contactref element="JP1" pad="6"/>
<contactref element="JP10" pad="1"/>
</signal>
<signal name="N$5">
<contactref element="U1" pad="7"/>
<contactref element="JP1" pad="7"/>
<contactref element="JP11" pad="1"/>
<contactref element="JP4" pad="2"/>
</signal>
<signal name="N$6">
<contactref element="U1" pad="12"/>
<contactref element="JP2" pad="5"/>
<contactref element="JP16" pad="1"/>
</signal>
<signal name="N$7">
<contactref element="U1" pad="11"/>
<contactref element="JP2" pad="6"/>
<contactref element="JP15" pad="1"/>
</signal>
<signal name="N$8">
<contactref element="U1" pad="13"/>
<contactref element="JP2" pad="4"/>
<contactref element="JP17" pad="1"/>
</signal>
<signal name="N$9">
<contactref element="U1" pad="10"/>
<contactref element="JP2" pad="7"/>
<contactref element="JP14" pad="1"/>
<contactref element="JP3" pad="2"/>
</signal>
<signal name="N$10">
<contactref element="U1" pad="14"/>
<contactref element="JP2" pad="3"/>
<contactref element="JP18" pad="1"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
